(kicad_pcb (version 20171130) (host pcbnew 5.1.6-c6e7f7d~87~ubuntu18.04.1)

  (general
    (thickness 1.6)
    (drawings 4)
    (tracks 176)
    (zones 0)
    (modules 12)
    (nets 39)
  )

  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )

  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.05)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )

  (net 0 "")
  (net 1 "Net-(A1-Pad16)")
  (net 2 "Net-(A1-Pad15)")
  (net 3 "Net-(A1-Pad30)")
  (net 4 "Net-(A1-Pad14)")
  (net 5 "Net-(A1-Pad29)")
  (net 6 "Net-(A1-Pad13)")
  (net 7 "Net-(A1-Pad28)")
  (net 8 "Net-(A1-Pad12)")
  (net 9 "Net-(A1-Pad27)")
  (net 10 "Net-(A1-Pad11)")
  (net 11 "Net-(A1-Pad26)")
  (net 12 "Net-(A1-Pad10)")
  (net 13 "Net-(A1-Pad25)")
  (net 14 "Net-(A1-Pad9)")
  (net 15 "Net-(A1-Pad24)")
  (net 16 "Net-(A1-Pad8)")
  (net 17 "Net-(A1-Pad23)")
  (net 18 "Net-(A1-Pad7)")
  (net 19 "Net-(A1-Pad22)")
  (net 20 "Net-(A1-Pad6)")
  (net 21 "Net-(A1-Pad21)")
  (net 22 "Net-(A1-Pad5)")
  (net 23 "Net-(A1-Pad20)")
  (net 24 "Net-(A1-Pad4)")
  (net 25 "Net-(A1-Pad19)")
  (net 26 "Net-(A1-Pad3)")
  (net 27 "Net-(A1-Pad18)")
  (net 28 "Net-(A1-Pad2)")
  (net 29 "Net-(A1-Pad17)")
  (net 30 "Net-(A1-Pad1)")
  (net 31 "Net-(U2-Pad5)")
  (net 32 "Net-(U2-Pad3)")
  (net 33 "Net-(U2-Pad2)")
  (net 34 "Net-(U2-Pad1)")
  (net 35 "Net-(U1-Pad8)")
  (net 36 "Net-(U2-Pad6)")
  (net 37 "Net-(D1-Pad1)")
  (net 38 "Net-(D1-Pad2)")

  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net "Net-(A1-Pad1)")
    (add_net "Net-(A1-Pad10)")
    (add_net "Net-(A1-Pad11)")
    (add_net "Net-(A1-Pad12)")
    (add_net "Net-(A1-Pad13)")
    (add_net "Net-(A1-Pad14)")
    (add_net "Net-(A1-Pad15)")
    (add_net "Net-(A1-Pad16)")
    (add_net "Net-(A1-Pad17)")
    (add_net "Net-(A1-Pad18)")
    (add_net "Net-(A1-Pad19)")
    (add_net "Net-(A1-Pad2)")
    (add_net "Net-(A1-Pad20)")
    (add_net "Net-(A1-Pad21)")
    (add_net "Net-(A1-Pad22)")
    (add_net "Net-(A1-Pad23)")
    (add_net "Net-(A1-Pad24)")
    (add_net "Net-(A1-Pad25)")
    (add_net "Net-(A1-Pad26)")
    (add_net "Net-(A1-Pad27)")
    (add_net "Net-(A1-Pad28)")
    (add_net "Net-(A1-Pad29)")
    (add_net "Net-(A1-Pad3)")
    (add_net "Net-(A1-Pad30)")
    (add_net "Net-(A1-Pad4)")
    (add_net "Net-(A1-Pad5)")
    (add_net "Net-(A1-Pad6)")
    (add_net "Net-(A1-Pad7)")
    (add_net "Net-(A1-Pad8)")
    (add_net "Net-(A1-Pad9)")
    (add_net "Net-(D1-Pad1)")
    (add_net "Net-(D1-Pad2)")
    (add_net "Net-(U1-Pad8)")
    (add_net "Net-(U2-Pad1)")
    (add_net "Net-(U2-Pad2)")
    (add_net "Net-(U2-Pad3)")
    (add_net "Net-(U2-Pad5)")
    (add_net "Net-(U2-Pad6)")
  )

  (module Diode_THT:D_A-405_P12.70mm_Horizontal (layer F.Cu) (tedit 5AE50CD5) (tstamp 5F6893B8)
    (at 200.406 125.73 90)
    (descr "Diode, A-405 series, Axial, Horizontal, pin pitch=12.7mm, , length*diameter=5.2*2.7mm^2, , http://www.diodes.com/_files/packages/A-405.pdf")
    (tags "Diode A-405 series Axial Horizontal pin pitch 12.7mm  length 5.2mm diameter 2.7mm")
    (path /5F6E4965)
    (fp_text reference D1 (at 6.35 -2.47 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value D_Schottky (at 6.35 2.47 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user K (at 0 -1.9 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user K (at 0 -1.9 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 6.74 0 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 3.75 -1.35) (end 3.75 1.35) (layer F.Fab) (width 0.1))
    (fp_line (start 3.75 1.35) (end 8.95 1.35) (layer F.Fab) (width 0.1))
    (fp_line (start 8.95 1.35) (end 8.95 -1.35) (layer F.Fab) (width 0.1))
    (fp_line (start 8.95 -1.35) (end 3.75 -1.35) (layer F.Fab) (width 0.1))
    (fp_line (start 0 0) (end 3.75 0) (layer F.Fab) (width 0.1))
    (fp_line (start 12.7 0) (end 8.95 0) (layer F.Fab) (width 0.1))
    (fp_line (start 4.53 -1.35) (end 4.53 1.35) (layer F.Fab) (width 0.1))
    (fp_line (start 4.63 -1.35) (end 4.63 1.35) (layer F.Fab) (width 0.1))
    (fp_line (start 4.43 -1.35) (end 4.43 1.35) (layer F.Fab) (width 0.1))
    (fp_line (start 3.63 -1.47) (end 3.63 1.47) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.63 1.47) (end 9.07 1.47) (layer F.SilkS) (width 0.12))
    (fp_line (start 9.07 1.47) (end 9.07 -1.47) (layer F.SilkS) (width 0.12))
    (fp_line (start 9.07 -1.47) (end 3.63 -1.47) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.14 0) (end 3.63 0) (layer F.SilkS) (width 0.12))
    (fp_line (start 11.56 0) (end 9.07 0) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.53 -1.47) (end 4.53 1.47) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.65 -1.47) (end 4.65 1.47) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.41 -1.47) (end 4.41 1.47) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.15 -1.6) (end -1.15 1.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.15 1.6) (end 13.85 1.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start 13.85 1.6) (end 13.85 -1.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start 13.85 -1.6) (end -1.15 -1.6) (layer F.CrtYd) (width 0.05))
    (pad 2 thru_hole oval (at 12.7 0 90) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 38 "Net-(D1-Pad2)"))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 37 "Net-(D1-Pad1)"))
    (model ${KISYS3DMOD}/Diode_THT.3dshapes/D_A-405_P12.70mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module cad-parts:18650-batt (layer B.Cu) (tedit 5F670EAD) (tstamp 5F684466)
    (at 153.924 114.3 180)
    (path /5F6CCA6F)
    (fp_text reference U4 (at 0.25 -3.25) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 18650-batt (at 0 8) (layer B.SilkS)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_line (start -38.5 10.5) (end 38.5 10.5) (layer B.SilkS) (width 0.12))
    (fp_line (start 38.5 10.5) (end 38.5 -10.5) (layer B.SilkS) (width 0.12))
    (fp_line (start 38.5 -10.5) (end -38.5 -10.5) (layer B.SilkS) (width 0.12))
    (fp_line (start -38.5 -10.5) (end -38.5 10.5) (layer B.SilkS) (width 0.12))
    (pad 2 thru_hole circle (at -36.25 0 180) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 38 "Net-(D1-Pad2)"))
    (pad 1 thru_hole circle (at 36.25 0 180) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 31 "Net-(U2-Pad5)"))
  )

  (module MountingHole:MountingHole_4mm (layer F.Cu) (tedit 56D1B4CB) (tstamp 5F67E8C6)
    (at 208.28 123.444)
    (descr "Mounting Hole 4mm, no annular")
    (tags "mounting hole 4mm no annular")
    (attr virtual)
    (fp_text reference REF** (at 0 -5) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value MountingHole_4mm (at 0 5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_circle (center 0 0) (end 4 0) (layer Cmts.User) (width 0.15))
    (fp_circle (center 0 0) (end 4.25 0) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 0.3 0) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 np_thru_hole circle (at 0 0) (size 4 4) (drill 4) (layers *.Cu *.Mask))
  )

  (module MountingHole:MountingHole_4mm (layer F.Cu) (tedit 56D1B4CB) (tstamp 5F67E8A6)
    (at 208.28 78.74)
    (descr "Mounting Hole 4mm, no annular")
    (tags "mounting hole 4mm no annular")
    (attr virtual)
    (fp_text reference REF** (at -7.62 -0.508) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value MountingHole_4mm (at 0 5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_circle (center 0 0) (end 4 0) (layer Cmts.User) (width 0.15))
    (fp_circle (center 0 0) (end 4.25 0) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 0.3 0) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 np_thru_hole circle (at 0 0) (size 4 4) (drill 4) (layers *.Cu *.Mask))
  )

  (module MountingHole:MountingHole_4mm (layer F.Cu) (tedit 56D1B4CB) (tstamp 5F67E8A6)
    (at 98.044 123.444)
    (descr "Mounting Hole 4mm, no annular")
    (tags "mounting hole 4mm no annular")
    (attr virtual)
    (fp_text reference REF** (at 0 -5) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value MountingHole_4mm (at 0 5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_circle (center 0 0) (end 4 0) (layer Cmts.User) (width 0.15))
    (fp_circle (center 0 0) (end 4.25 0) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 0.3 0) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 np_thru_hole circle (at 0 0) (size 4 4) (drill 4) (layers *.Cu *.Mask))
  )

  (module MountingHole:MountingHole_4mm (layer F.Cu) (tedit 56D1B4CB) (tstamp 5F67E649)
    (at 98.044 78.74)
    (descr "Mounting Hole 4mm, no annular")
    (tags "mounting hole 4mm no annular")
    (attr virtual)
    (fp_text reference REF** (at 0 -5) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value MountingHole_4mm (at 0 5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0.3 0) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_circle (center 0 0) (end 4 0) (layer Cmts.User) (width 0.15))
    (fp_circle (center 0 0) (end 4.25 0) (layer F.CrtYd) (width 0.05))
    (pad 1 np_thru_hole circle (at 0 0) (size 4 4) (drill 4) (layers *.Cu *.Mask))
  )

  (module cad-parts:nRF24 (layer F.Cu) (tedit 5F66FAA4) (tstamp 5F67CB84)
    (at 152.4 100.33)
    (path /5F508671)
    (fp_text reference U1 (at -5.91 0 90) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value nRF24 (at 0 -3.81) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -5.5 -25) (end 8.5 -25) (layer F.SilkS) (width 0.12))
    (fp_line (start -5.5 2.5) (end -5.5 -25) (layer F.SilkS) (width 0.12))
    (fp_line (start 8.5 3) (end 8.5 -25) (layer F.SilkS) (width 0.12))
    (fp_line (start -5.5 3) (end 8.5 3) (layer F.SilkS) (width 0.12))
    (fp_line (start -5.5 2.5) (end -5.5 3) (layer F.SilkS) (width 0.12))
    (fp_line (start -4.66 -2.52) (end 4.66 -2.52) (layer F.CrtYd) (width 0.05))
    (fp_line (start 4.66 -2.52) (end 4.66 2.52) (layer F.CrtYd) (width 0.05))
    (fp_line (start 4.66 2.52) (end -4.66 2.52) (layer F.CrtYd) (width 0.05))
    (fp_line (start -4.66 2.52) (end -4.66 -2.52) (layer F.CrtYd) (width 0.05))
    (pad 7 thru_hole oval (at 3.81 1.27) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "Net-(A1-Pad15)"))
    (pad 8 thru_hole oval (at 3.81 -1.27) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 35 "Net-(U1-Pad8)"))
    (pad 5 thru_hole oval (at 1.27 1.27) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 "Net-(A1-Pad16)"))
    (pad 6 thru_hole oval (at 1.27 -1.27) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 "Net-(A1-Pad14)"))
    (pad 3 thru_hole oval (at -1.27 1.27) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 12 "Net-(A1-Pad10)"))
    (pad 4 thru_hole oval (at -1.27 -1.27) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 10 "Net-(A1-Pad11)"))
    (pad 1 thru_hole oval (at -3.81 1.27) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 "Net-(A1-Pad29)"))
    (pad 2 thru_hole oval (at -3.81 -1.27) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 29 "Net-(A1-Pad17)"))
  )

  (module cad-parts:dc-converter (layer F.Cu) (tedit 5F66F47D) (tstamp 5F67A875)
    (at 166.37 116.84)
    (path /5F69BA43)
    (fp_text reference U3 (at 0.5 1.5) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value dc-converter (at 0.25 -1) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -18.25 -8.5) (end 18.25 -8.5) (layer F.SilkS) (width 0.12))
    (fp_line (start 18.25 -8.5) (end 18.25 8) (layer F.SilkS) (width 0.12))
    (fp_line (start -18.25 -8.5) (end -18.25 8) (layer F.SilkS) (width 0.12))
    (fp_line (start -18.25 8) (end 18.25 8) (layer F.SilkS) (width 0.12))
    (pad 4 thru_hole circle (at -15.25 3.75) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 5 "Net-(A1-Pad29)"))
    (pad 3 thru_hole circle (at -15.25 -3.75) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 3 "Net-(A1-Pad30)"))
    (pad 2 thru_hole circle (at 15.25 3.75) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 36 "Net-(U2-Pad6)"))
    (pad 1 thru_hole circle (at 15.25 -3.75) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 32 "Net-(U2-Pad3)"))
  )

  (module cad-parts:TC4056A-MOD (layer F.Cu) (tedit 5F66FC85) (tstamp 5F678EC7)
    (at 173.99 88.9)
    (path /5F679D5C)
    (fp_text reference U2 (at 0.254 -11.684) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value TC4056-MOD (at 0 -17.25) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 0 -14) (end 8.5 -14) (layer F.SilkS) (width 0.12))
    (fp_line (start 8.5 -14) (end 0 -14) (layer F.SilkS) (width 0.12))
    (fp_line (start 0 -14) (end -8.5 -14) (layer F.SilkS) (width 0.12))
    (fp_line (start -8.5 -14) (end -8.5 14) (layer F.SilkS) (width 0.12))
    (fp_line (start 8.5 -14) (end 8.5 14) (layer F.SilkS) (width 0.12))
    (fp_line (start 8.5 14) (end -8.5 14) (layer F.SilkS) (width 0.12))
    (pad 5 thru_hole circle (at -3.75 10) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 31 "Net-(U2-Pad5)"))
    (pad 6 thru_hole circle (at -7 10) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 36 "Net-(U2-Pad6)"))
    (pad 4 thru_hole circle (at 3.75 10) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 37 "Net-(D1-Pad1)"))
    (pad 3 thru_hole circle (at 7 10) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 32 "Net-(U2-Pad3)"))
    (pad 2 thru_hole circle (at 7 -12.5) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 33 "Net-(U2-Pad2)"))
    (pad 1 thru_hole circle (at -7 -12.5) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 34 "Net-(U2-Pad1)"))
  )

  (module Module:Arduino_Nano (layer F.Cu) (tedit 58ACAF70) (tstamp 5F50ECE2)
    (at 140.97 114.3 180)
    (descr "Arduino Nano, http://www.mouser.com/pdfdocs/Gravitech_Arduino_Nano3_0.pdf")
    (tags "Arduino Nano")
    (path /5F50914A)
    (fp_text reference A1 (at 7.62 -5.08) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value Arduino_Nano_v2.x (at 8.89 19.05 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.27 1.27) (end 1.27 -1.27) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.27 -1.27) (end -1.4 -1.27) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.4 1.27) (end -1.4 39.5) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.4 -3.94) (end -1.4 -1.27) (layer F.SilkS) (width 0.12))
    (fp_line (start 13.97 -1.27) (end 16.64 -1.27) (layer F.SilkS) (width 0.12))
    (fp_line (start 13.97 -1.27) (end 13.97 36.83) (layer F.SilkS) (width 0.12))
    (fp_line (start 13.97 36.83) (end 16.64 36.83) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.27 1.27) (end -1.4 1.27) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.27 1.27) (end 1.27 36.83) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.27 36.83) (end -1.4 36.83) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.81 31.75) (end 11.43 31.75) (layer F.Fab) (width 0.1))
    (fp_line (start 11.43 31.75) (end 11.43 41.91) (layer F.Fab) (width 0.1))
    (fp_line (start 11.43 41.91) (end 3.81 41.91) (layer F.Fab) (width 0.1))
    (fp_line (start 3.81 41.91) (end 3.81 31.75) (layer F.Fab) (width 0.1))
    (fp_line (start -1.4 39.5) (end 16.64 39.5) (layer F.SilkS) (width 0.12))
    (fp_line (start 16.64 39.5) (end 16.64 -3.94) (layer F.SilkS) (width 0.12))
    (fp_line (start 16.64 -3.94) (end -1.4 -3.94) (layer F.SilkS) (width 0.12))
    (fp_line (start 16.51 39.37) (end -1.27 39.37) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 39.37) (end -1.27 -2.54) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 -2.54) (end 0 -3.81) (layer F.Fab) (width 0.1))
    (fp_line (start 0 -3.81) (end 16.51 -3.81) (layer F.Fab) (width 0.1))
    (fp_line (start 16.51 -3.81) (end 16.51 39.37) (layer F.Fab) (width 0.1))
    (fp_line (start -1.53 -4.06) (end 16.75 -4.06) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.53 -4.06) (end -1.53 42.16) (layer F.CrtYd) (width 0.05))
    (fp_line (start 16.75 42.16) (end 16.75 -4.06) (layer F.CrtYd) (width 0.05))
    (fp_line (start 16.75 42.16) (end -1.53 42.16) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 6.35 19.05 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 16 thru_hole oval (at 15.24 35.56 180) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 1 "Net-(A1-Pad16)"))
    (pad 15 thru_hole oval (at 0 35.56 180) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 2 "Net-(A1-Pad15)"))
    (pad 30 thru_hole oval (at 15.24 0 180) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 3 "Net-(A1-Pad30)"))
    (pad 14 thru_hole oval (at 0 33.02 180) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 4 "Net-(A1-Pad14)"))
    (pad 29 thru_hole oval (at 15.24 2.54 180) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 5 "Net-(A1-Pad29)"))
    (pad 13 thru_hole oval (at 0 30.48 180) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 6 "Net-(A1-Pad13)"))
    (pad 28 thru_hole oval (at 15.24 5.08 180) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 7 "Net-(A1-Pad28)"))
    (pad 12 thru_hole oval (at 0 27.94 180) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 8 "Net-(A1-Pad12)"))
    (pad 27 thru_hole oval (at 15.24 7.62 180) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 9 "Net-(A1-Pad27)"))
    (pad 11 thru_hole oval (at 0 25.4 180) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 10 "Net-(A1-Pad11)"))
    (pad 26 thru_hole oval (at 15.24 10.16 180) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 11 "Net-(A1-Pad26)"))
    (pad 10 thru_hole oval (at 0 22.86 180) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 12 "Net-(A1-Pad10)"))
    (pad 25 thru_hole oval (at 15.24 12.7 180) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 13 "Net-(A1-Pad25)"))
    (pad 9 thru_hole oval (at 0 20.32 180) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 14 "Net-(A1-Pad9)"))
    (pad 24 thru_hole oval (at 15.24 15.24 180) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 15 "Net-(A1-Pad24)"))
    (pad 8 thru_hole oval (at 0 17.78 180) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 16 "Net-(A1-Pad8)"))
    (pad 23 thru_hole oval (at 15.24 17.78 180) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 17 "Net-(A1-Pad23)"))
    (pad 7 thru_hole oval (at 0 15.24 180) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 18 "Net-(A1-Pad7)"))
    (pad 22 thru_hole oval (at 15.24 20.32 180) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 19 "Net-(A1-Pad22)"))
    (pad 6 thru_hole oval (at 0 12.7 180) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 20 "Net-(A1-Pad6)"))
    (pad 21 thru_hole oval (at 15.24 22.86 180) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 21 "Net-(A1-Pad21)"))
    (pad 5 thru_hole oval (at 0 10.16 180) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 22 "Net-(A1-Pad5)"))
    (pad 20 thru_hole oval (at 15.24 25.4 180) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 23 "Net-(A1-Pad20)"))
    (pad 4 thru_hole oval (at 0 7.62 180) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 24 "Net-(A1-Pad4)"))
    (pad 19 thru_hole oval (at 15.24 27.94 180) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 25 "Net-(A1-Pad19)"))
    (pad 3 thru_hole oval (at 0 5.08 180) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 26 "Net-(A1-Pad3)"))
    (pad 18 thru_hole oval (at 15.24 30.48 180) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 27 "Net-(A1-Pad18)"))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 28 "Net-(A1-Pad2)"))
    (pad 17 thru_hole oval (at 15.24 33.02 180) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 29 "Net-(A1-Pad17)"))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 30 "Net-(A1-Pad1)"))
    (model ${KISYS3DMOD}/Module.3dshapes/Arduino_Nano_WithMountingHoles.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module cad-parts:JOYSTICK-ALPS (layer F.Cu) (tedit 5F508F32) (tstamp 5F50F288)
    (at 106.68 99.06)
    (path /5F50A4B2)
    (attr virtual)
    (fp_text reference J1 (at -1.905 4.445) (layer B.SilkS) hide
      (effects (font (size 1.27 1.27) (thickness 0.1016)))
    )
    (fp_text value JOYSTICK-ALPS (at -0.254 1.524) (layer B.SilkS) hide
      (effects (font (size 1.27 1.27) (thickness 0.1016)))
    )
    (fp_circle (center 0 0) (end -6.35 6.35) (layer F.SilkS) (width 0.1016))
    (fp_circle (center 0 0) (end -0.3175 0.3175) (layer B.SilkS) (width 0.1016))
    (fp_line (start 0.635 -5.84) (end 1.905 -5.84) (layer F.SilkS) (width 0.2032))
    (fp_line (start -0.635 -5.84) (end 0.635 -6.475) (layer F.SilkS) (width 0.2032))
    (fp_line (start -1.905 -5.84) (end -0.635 -5.84) (layer F.SilkS) (width 0.2032))
    (fp_line (start -7.62 4.826) (end -7.62 8.89) (layer B.SilkS) (width 0.2032))
    (fp_line (start -7.62 -4.826) (end -7.62 -6.985) (layer B.SilkS) (width 0.2032))
    (fp_line (start -11.176 -4.826) (end -11.176 4.826) (layer B.SilkS) (width 0.2032))
    (fp_line (start -7.62 4.826) (end -11.176 4.826) (layer B.SilkS) (width 0.2032))
    (fp_line (start -7.62 -4.826) (end -11.176 -4.826) (layer B.SilkS) (width 0.2032))
    (fp_line (start -5.588 -12) (end -5.588 -6.985) (layer B.SilkS) (width 0.2032))
    (fp_line (start 5.588 -12) (end 5.588 -6.985) (layer B.SilkS) (width 0.2032))
    (fp_line (start -5.588 -6.985) (end -7.62 -6.985) (layer B.SilkS) (width 0.2032))
    (fp_line (start 7.62 -6.985) (end 5.588 -6.985) (layer B.SilkS) (width 0.2032))
    (fp_line (start 7.62 4.064) (end 9.525 4.064) (layer B.SilkS) (width 0.2032))
    (fp_line (start 7.62 -4.064) (end 9.525 -4.064) (layer B.SilkS) (width 0.2032))
    (fp_line (start 7.62 4.064) (end 7.62 8.89) (layer B.SilkS) (width 0.2032))
    (fp_line (start 7.62 -4.064) (end 7.62 -6.985) (layer B.SilkS) (width 0.2032))
    (fp_line (start 9.525 -4.064) (end 9.525 4.064) (layer B.SilkS) (width 0.2032))
    (fp_line (start -4.826 8.89) (end -7.62 8.89) (layer B.SilkS) (width 0.2032))
    (fp_line (start 4.826 8.89) (end 7.62 8.89) (layer B.SilkS) (width 0.2032))
    (fp_line (start -4.826 11.43) (end -4.826 8.89) (layer B.SilkS) (width 0.2032))
    (fp_line (start 4.826 11.43) (end 4.826 8.89) (layer B.SilkS) (width 0.2032))
    (fp_line (start 4.826 11.43) (end -4.826 11.43) (layer B.SilkS) (width 0.2032))
    (fp_line (start 5.588 -12) (end -5.588 -12) (layer B.SilkS) (width 0.2032))
    (pad 4 thru_hole circle (at -8.73 2.55) (size 1.778 1.778) (drill 1) (layers *.Cu F.Paste F.SilkS F.Mask)
      (net 5 "Net-(A1-Pad29)"))
    (pad 1 thru_hole circle (at -8.73 0) (size 1.778 1.778) (drill 1) (layers *.Cu F.Paste F.SilkS F.Mask)
      (net 15 "Net-(A1-Pad24)"))
    (pad 0 thru_hole circle (at -8.732 -2.55) (size 1.778 1.778) (drill 1) (layers *.Cu F.Paste F.SilkS F.Mask)
      (net 29 "Net-(A1-Pad17)"))
    (pad MOUN thru_hole circle (at 6.325 -5) (size 2.286 2.286) (drill 1.5) (layers *.Cu F.Paste F.SilkS F.Mask))
    (pad MOUN thru_hole circle (at 6.325 5) (size 2.286 2.286) (drill 1.5) (layers *.Cu F.Paste F.SilkS F.Mask))
    (pad 0 thru_hole circle (at -6.325 5) (size 2.286 2.286) (drill 1.5) (layers *.Cu F.Paste F.SilkS F.Mask)
      (net 29 "Net-(A1-Pad17)"))
    (pad MOUN thru_hole circle (at -6.325 -5) (size 2.286 2.286) (drill 1.5) (layers *.Cu F.Paste F.SilkS F.Mask))
    (pad 4 thru_hole circle (at 2.55 8.73) (size 1.778 1.778) (drill 1) (layers *.Cu F.Paste F.SilkS F.Mask)
      (net 5 "Net-(A1-Pad29)"))
    (pad 2 thru_hole circle (at 0 8.73) (size 1.778 1.778) (drill 1) (layers *.Cu F.Paste F.SilkS F.Mask)
      (net 17 "Net-(A1-Pad23)"))
    (pad 0 thru_hole circle (at -2.55 8.73) (size 1.778 1.778) (drill 1) (layers *.Cu F.Paste F.SilkS F.Mask)
      (net 29 "Net-(A1-Pad17)"))
    (pad 4 thru_hole circle (at 3.25 -5.75) (size 1.778 1.778) (drill 1.2) (layers *.Cu F.Paste F.SilkS F.Mask)
      (net 5 "Net-(A1-Pad29)"))
    (pad 4 thru_hole circle (at -3.25 -5.75) (size 1.778 1.778) (drill 1.2) (layers *.Cu F.Paste F.SilkS F.Mask)
      (net 5 "Net-(A1-Pad29)"))
    (pad 3 thru_hole circle (at 3.25 -10.25) (size 1.778 1.778) (drill 1.2) (layers *.Cu F.Paste F.SilkS F.Mask)
      (net 8 "Net-(A1-Pad12)"))
    (pad 3 thru_hole circle (at -3.25 -10.25) (size 1.778 1.778) (drill 1.2) (layers *.Cu F.Paste F.SilkS F.Mask)
      (net 8 "Net-(A1-Pad12)"))
  )

  (module cad-parts:JOYSTICK-ALPS (layer F.Cu) (tedit 5F51AB0B) (tstamp 5F51ACDE)
    (at 201.93 99.06)
    (path /5F510B0B)
    (attr virtual)
    (fp_text reference J2 (at -1.905 4.445) (layer F.SilkS)
      (effects (font (size 1.27 1.27) (thickness 0.1016)))
    )
    (fp_text value JOYSTICK-ALPS (at -1.27 5.715) (layer F.SilkS) hide
      (effects (font (size 1.27 1.27) (thickness 0.1016)))
    )
    (fp_circle (center 0 0) (end -6.35 6.35) (layer F.SilkS) (width 0.1016))
    (fp_circle (center 0 0) (end -0.3175 0.3175) (layer B.SilkS) (width 0.1016))
    (fp_line (start 0.635 -5.84) (end 1.905 -5.84) (layer F.SilkS) (width 0.2032))
    (fp_line (start -0.635 -5.84) (end 0.635 -6.475) (layer F.SilkS) (width 0.2032))
    (fp_line (start -1.905 -5.84) (end -0.635 -5.84) (layer F.SilkS) (width 0.2032))
    (fp_line (start -7.62 4.826) (end -7.62 8.89) (layer B.SilkS) (width 0.2032))
    (fp_line (start -7.62 -4.826) (end -7.62 -6.985) (layer B.SilkS) (width 0.2032))
    (fp_line (start -11.176 -4.826) (end -11.176 4.826) (layer B.SilkS) (width 0.2032))
    (fp_line (start -7.62 4.826) (end -11.176 4.826) (layer B.SilkS) (width 0.2032))
    (fp_line (start -7.62 -4.826) (end -11.176 -4.826) (layer B.SilkS) (width 0.2032))
    (fp_line (start -5.588 -12) (end -5.588 -6.985) (layer B.SilkS) (width 0.2032))
    (fp_line (start 5.588 -12) (end 5.588 -6.985) (layer B.SilkS) (width 0.2032))
    (fp_line (start -5.588 -6.985) (end -7.62 -6.985) (layer B.SilkS) (width 0.2032))
    (fp_line (start 7.62 -6.985) (end 5.588 -6.985) (layer B.SilkS) (width 0.2032))
    (fp_line (start 7.62 4.064) (end 9.525 4.064) (layer B.SilkS) (width 0.2032))
    (fp_line (start 7.62 -4.064) (end 9.525 -4.064) (layer B.SilkS) (width 0.2032))
    (fp_line (start 7.62 4.064) (end 7.62 8.89) (layer B.SilkS) (width 0.2032))
    (fp_line (start 7.62 -4.064) (end 7.62 -6.985) (layer B.SilkS) (width 0.2032))
    (fp_line (start 9.525 -4.064) (end 9.525 4.064) (layer B.SilkS) (width 0.2032))
    (fp_line (start -4.826 8.89) (end -7.62 8.89) (layer B.SilkS) (width 0.2032))
    (fp_line (start 4.826 8.89) (end 7.62 8.89) (layer B.SilkS) (width 0.2032))
    (fp_line (start -4.826 11.43) (end -4.826 8.89) (layer B.SilkS) (width 0.2032))
    (fp_line (start 4.826 11.43) (end 4.826 8.89) (layer B.SilkS) (width 0.2032))
    (fp_line (start 4.826 11.43) (end -4.826 11.43) (layer B.SilkS) (width 0.2032))
    (fp_line (start 5.588 -12) (end -5.588 -12) (layer B.SilkS) (width 0.2032))
    (pad 4 thru_hole circle (at -8.73 2.55) (size 1.778 1.778) (drill 1) (layers *.Cu F.Paste F.SilkS F.Mask)
      (net 5 "Net-(A1-Pad29)"))
    (pad 1 thru_hole circle (at -8.73 0) (size 1.778 1.778) (drill 1) (layers *.Cu F.Paste F.SilkS F.Mask)
      (net 13 "Net-(A1-Pad25)"))
    (pad 0 thru_hole circle (at -8.732 -2.55) (size 1.778 1.778) (drill 1) (layers *.Cu F.Paste F.SilkS F.Mask)
      (net 29 "Net-(A1-Pad17)"))
    (pad MOUN thru_hole circle (at 6.325 -5) (size 2.286 2.286) (drill 1.5) (layers *.Cu F.Paste F.SilkS F.Mask))
    (pad MOUN thru_hole circle (at 6.325 5) (size 2.286 2.286) (drill 1.5) (layers *.Cu F.Paste F.SilkS F.Mask))
    (pad 0 thru_hole circle (at -6.325 5) (size 2.286 2.286) (drill 1.5) (layers *.Cu F.Paste F.SilkS F.Mask)
      (net 29 "Net-(A1-Pad17)"))
    (pad MOUN thru_hole circle (at -6.325 -5) (size 2.286 2.286) (drill 1.5) (layers *.Cu F.Paste F.SilkS F.Mask))
    (pad 4 thru_hole circle (at 2.55 8.73) (size 1.778 1.778) (drill 1) (layers *.Cu F.Paste F.SilkS F.Mask)
      (net 5 "Net-(A1-Pad29)"))
    (pad 2 thru_hole circle (at 0 8.73) (size 1.778 1.778) (drill 1) (layers *.Cu F.Paste F.SilkS F.Mask)
      (net 11 "Net-(A1-Pad26)"))
    (pad 0 thru_hole circle (at -2.55 8.73) (size 1.778 1.778) (drill 1) (layers *.Cu F.Paste F.SilkS F.Mask)
      (net 29 "Net-(A1-Pad17)"))
    (pad 4 thru_hole circle (at 3.25 -5.75) (size 1.778 1.778) (drill 1.2) (layers *.Cu F.Paste F.SilkS F.Mask)
      (net 5 "Net-(A1-Pad29)"))
    (pad 4 thru_hole circle (at -3.25 -5.75) (size 1.778 1.778) (drill 1.2) (layers *.Cu F.Paste F.SilkS F.Mask)
      (net 5 "Net-(A1-Pad29)"))
    (pad 3 thru_hole circle (at 3.25 -10.25) (size 1.778 1.778) (drill 1.2) (layers *.Cu F.Paste F.SilkS F.Mask)
      (net 6 "Net-(A1-Pad13)"))
    (pad 3 thru_hole circle (at -3.25 -10.25) (size 1.778 1.778) (drill 1.2) (layers *.Cu F.Paste F.SilkS F.Mask)
      (net 6 "Net-(A1-Pad13)"))
  )

  (gr_line (start 93.472 128.016) (end 93.472 74.168) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 212.852 128.016) (end 93.472 128.016) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 212.852 74.168) (end 212.852 128.016) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 93.472 74.168) (end 212.852 74.168) (layer Edge.Cuts) (width 0.05))

  (segment (start 153.67 101.6) (end 154.94 100.33) (width 0.25) (layer F.Cu) (net 1))
  (segment (start 154.94 100.33) (end 154.94 86.36) (width 0.25) (layer F.Cu) (net 1))
  (segment (start 154.94 86.36) (end 154.94 78.74) (width 0.25) (layer F.Cu) (net 1))
  (segment (start 154.94 78.74) (end 154.94 77.47) (width 0.25) (layer F.Cu) (net 1))
  (segment (start 154.94 77.47) (end 153.67 76.2) (width 0.25) (layer F.Cu) (net 1))
  (segment (start 125.73 78.74) (end 127 78.74) (width 0.25) (layer F.Cu) (net 1))
  (segment (start 127 78.74) (end 129.54 76.2) (width 0.25) (layer F.Cu) (net 1))
  (segment (start 129.54 76.2) (end 153.67 76.2) (width 0.25) (layer F.Cu) (net 1))
  (segment (start 156.21 101.6) (end 157.48 100.33) (width 0.25) (layer F.Cu) (net 2))
  (segment (start 157.48 100.33) (end 157.48 95.25) (width 0.25) (layer F.Cu) (net 2))
  (segment (start 157.48 95.25) (end 157.48 78.74) (width 0.25) (layer F.Cu) (net 2))
  (segment (start 140.97 78.74) (end 147.32 78.74) (width 0.25) (layer F.Cu) (net 2))
  (segment (start 157.48 78.74) (end 157.48 78.74) (width 0.25) (layer F.Cu) (net 2) (tstamp 5F67D397))
  (via (at 157.48 78.74) (size 0.8) (drill 0.4) (layers F.Cu B.Cu) (net 2))
  (segment (start 147.32 78.74) (end 147.32 78.74) (width 0.25) (layer F.Cu) (net 2) (tstamp 5F67D39F))
  (via (at 147.32 78.74) (size 0.8) (drill 0.4) (layers F.Cu B.Cu) (net 2))
  (segment (start 157.48 78.74) (end 147.32 78.74) (width 0.25) (layer B.Cu) (net 2))
  (segment (start 132.08 123.19) (end 125.73 116.84) (width 0.25) (layer F.Cu) (net 3))
  (segment (start 125.73 114.3) (end 125.73 116.84) (width 0.25) (layer F.Cu) (net 3))
  (segment (start 132.08 123.19) (end 152.4 123.19) (width 0.25) (layer F.Cu) (net 3))
  (segment (start 152.4 114.37) (end 151.12 113.09) (width 0.25) (layer F.Cu) (net 3))
  (segment (start 152.4 123.19) (end 152.4 114.37) (width 0.25) (layer F.Cu) (net 3))
  (segment (start 153.67 99.06) (end 153.67 81.28) (width 0.25) (layer F.Cu) (net 4))
  (segment (start 140.97 81.28) (end 147.32 81.28) (width 0.25) (layer F.Cu) (net 4))
  (segment (start 153.67 81.28) (end 153.67 81.28) (width 0.25) (layer F.Cu) (net 4) (tstamp 5F67D39B))
  (via (at 153.67 81.28) (size 0.8) (drill 0.4) (layers F.Cu B.Cu) (net 4))
  (segment (start 147.32 81.28) (end 147.32 81.28) (width 0.25) (layer F.Cu) (net 4) (tstamp 5F67D39D))
  (via (at 147.32 81.28) (size 0.8) (drill 0.4) (layers F.Cu B.Cu) (net 4))
  (segment (start 147.32 81.28) (end 153.67 81.28) (width 0.25) (layer B.Cu) (net 4))
  (segment (start 97.95 103.827642) (end 103.126359 109.004001) (width 0.25) (layer F.Cu) (net 5))
  (segment (start 108.015999 109.004001) (end 109.23 107.79) (width 0.25) (layer F.Cu) (net 5))
  (segment (start 97.95 101.61) (end 97.95 103.827642) (width 0.25) (layer F.Cu) (net 5))
  (segment (start 109.93 93.31) (end 103.43 93.31) (width 0.25) (layer F.Cu) (net 5))
  (segment (start 198.68 93.31) (end 205.18 93.31) (width 0.25) (layer F.Cu) (net 5))
  (segment (start 204.48 94.01) (end 205.18 93.31) (width 0.25) (layer F.Cu) (net 5))
  (segment (start 204.48 107.79) (end 204.48 99.05) (width 0.25) (layer F.Cu) (net 5))
  (segment (start 133.35 121.92) (end 147.32 121.92) (width 0.25) (layer F.Cu) (net 5))
  (segment (start 109.23 107.79) (end 112.87 107.79) (width 0.25) (layer F.Cu) (net 5))
  (segment (start 112.87 107.79) (end 113.03 107.95) (width 0.25) (layer F.Cu) (net 5))
  (segment (start 105.344001 108.854001) (end 105.194001 109.004001) (width 0.25) (layer F.Cu) (net 5))
  (segment (start 105.344001 97.895999) (end 105.344001 108.854001) (width 0.25) (layer F.Cu) (net 5))
  (segment (start 109.93 93.31) (end 105.344001 97.895999) (width 0.25) (layer F.Cu) (net 5))
  (segment (start 103.126359 109.004001) (end 105.194001 109.004001) (width 0.25) (layer F.Cu) (net 5))
  (segment (start 105.194001 109.004001) (end 108.015999 109.004001) (width 0.25) (layer F.Cu) (net 5))
  (segment (start 125.73 111.76) (end 116.84 111.76) (width 0.25) (layer F.Cu) (net 5))
  (segment (start 116.84 111.76) (end 113.03 107.95) (width 0.25) (layer F.Cu) (net 5))
  (segment (start 133.35 119.38) (end 133.35 121.92) (width 0.25) (layer F.Cu) (net 5))
  (segment (start 125.73 111.76) (end 133.35 119.38) (width 0.25) (layer F.Cu) (net 5))
  (segment (start 149.040009 104.590009) (end 148.59 104.14) (width 0.25) (layer F.Cu) (net 5))
  (segment (start 148.59 101.6) (end 148.59 104.14) (width 0.25) (layer F.Cu) (net 5))
  (segment (start 193.2 101.61) (end 190.575 98.985) (width 0.25) (layer F.Cu) (net 5))
  (segment (start 188.55001 96.96001) (end 165.2964 96.96001) (width 0.25) (layer F.Cu) (net 5))
  (segment (start 165.2964 96.96001) (end 157.666401 104.590009) (width 0.25) (layer F.Cu) (net 5))
  (segment (start 157.666401 104.590009) (end 149.040009 104.590009) (width 0.25) (layer F.Cu) (net 5))
  (segment (start 148.59 118.06) (end 151.12 120.59) (width 0.25) (layer F.Cu) (net 5))
  (segment (start 148.59 104.14) (end 148.59 118.06) (width 0.25) (layer F.Cu) (net 5))
  (segment (start 151.12 120.59) (end 148.65 120.59) (width 0.25) (layer F.Cu) (net 5))
  (segment (start 148.65 120.59) (end 147.32 121.92) (width 0.25) (layer F.Cu) (net 5))
  (segment (start 190.575 98.985) (end 188.55001 96.96001) (width 0.25) (layer F.Cu) (net 5) (tstamp 5F67D393))
  (via (at 190.575 98.985) (size 0.8) (drill 0.4) (layers F.Cu B.Cu) (net 5))
  (segment (start 204.48 99.05) (end 204.48 94.01) (width 0.25) (layer F.Cu) (net 5) (tstamp 5F67D395))
  (via (at 204.48 99.05) (size 0.8) (drill 0.4) (layers F.Cu B.Cu) (net 5))
  (segment (start 203.275999 97.845999) (end 204.48 99.05) (width 0.25) (layer B.Cu) (net 5))
  (segment (start 191.714001 97.845999) (end 203.275999 97.845999) (width 0.25) (layer B.Cu) (net 5))
  (segment (start 190.575 98.985) (end 191.714001 97.845999) (width 0.25) (layer B.Cu) (net 5))
  (segment (start 205.18 88.81) (end 198.68 88.81) (width 0.25) (layer F.Cu) (net 6))
  (segment (start 140.97 83.82) (end 147.32 83.82) (width 0.25) (layer F.Cu) (net 6))
  (segment (start 198.68 88.81) (end 163.74 88.81) (width 0.25) (layer F.Cu) (net 6))
  (segment (start 163.74 88.81) (end 158.75 83.82) (width 0.25) (layer F.Cu) (net 6))
  (segment (start 158.75 83.82) (end 158.75 83.82) (width 0.25) (layer F.Cu) (net 6) (tstamp 5F67D399))
  (via (at 158.75 83.82) (size 0.8) (drill 0.4) (layers F.Cu B.Cu) (net 6))
  (segment (start 147.32 83.82) (end 147.32 83.82) (width 0.25) (layer F.Cu) (net 6) (tstamp 5F67D3A1))
  (via (at 147.32 83.82) (size 0.8) (drill 0.4) (layers F.Cu B.Cu) (net 6))
  (segment (start 158.75 83.82) (end 147.32 83.82) (width 0.25) (layer B.Cu) (net 6))
  (segment (start 103.43 88.81) (end 109.93 88.81) (width 0.25) (layer F.Cu) (net 8))
  (segment (start 139.844999 87.485001) (end 140.97 86.36) (width 0.25) (layer F.Cu) (net 8))
  (segment (start 111.254999 87.485001) (end 139.844999 87.485001) (width 0.25) (layer F.Cu) (net 8))
  (segment (start 109.93 88.81) (end 111.254999 87.485001) (width 0.25) (layer F.Cu) (net 8))
  (segment (start 140.97 88.9) (end 147.32 88.9) (width 0.25) (layer F.Cu) (net 10))
  (segment (start 151.13 99.06) (end 151.13 88.9) (width 0.25) (layer F.Cu) (net 10))
  (segment (start 147.32 88.9) (end 147.32 88.9) (width 0.25) (layer F.Cu) (net 10) (tstamp 5F67D3A3))
  (via (at 147.32 88.9) (size 0.8) (drill 0.4) (layers F.Cu B.Cu) (net 10))
  (segment (start 151.13 88.9) (end 151.13 88.9) (width 0.25) (layer F.Cu) (net 10) (tstamp 5F67D3A7))
  (via (at 151.13 88.9) (size 0.8) (drill 0.4) (layers F.Cu B.Cu) (net 10))
  (segment (start 151.13 88.9) (end 147.32 88.9) (width 0.25) (layer B.Cu) (net 10))
  (segment (start 201.93 107.79) (end 182.72 127) (width 0.25) (layer F.Cu) (net 11))
  (segment (start 182.72 127) (end 129.54 127) (width 0.25) (layer F.Cu) (net 11))
  (segment (start 129.54 127) (end 121.92 119.38) (width 0.25) (layer F.Cu) (net 11))
  (segment (start 121.92 119.38) (end 121.92 115.57) (width 0.25) (layer F.Cu) (net 11))
  (segment (start 121.92 107.95) (end 121.92 110.49) (width 0.25) (layer F.Cu) (net 11))
  (segment (start 121.92 115.57) (end 121.92 115.57) (width 0.25) (layer F.Cu) (net 11) (tstamp 5F67B297))
  (via (at 121.92 115.57) (size 0.8) (drill 0.4) (layers F.Cu B.Cu) (net 11))
  (via (at 121.92 110.49) (size 0.8) (drill 0.4) (layers F.Cu B.Cu) (net 11))
  (segment (start 121.92 107.95) (end 125.73 104.14) (width 0.25) (layer F.Cu) (net 11))
  (segment (start 121.92 115.57) (end 121.92 110.49) (width 0.25) (layer B.Cu) (net 11))
  (segment (start 151.13 101.6) (end 152.4 100.33) (width 0.25) (layer F.Cu) (net 12))
  (segment (start 152.4 100.33) (end 152.4 92.71) (width 0.25) (layer F.Cu) (net 12))
  (segment (start 152.4 92.71) (end 152.4 91.44) (width 0.25) (layer F.Cu) (net 12))
  (segment (start 140.97 91.44) (end 147.32 91.44) (width 0.25) (layer F.Cu) (net 12))
  (segment (start 147.32 91.44) (end 147.32 91.44) (width 0.25) (layer F.Cu) (net 12) (tstamp 5F67D3A5))
  (via (at 147.32 91.44) (size 0.8) (drill 0.4) (layers F.Cu B.Cu) (net 12))
  (segment (start 152.4 91.44) (end 152.4 91.44) (width 0.25) (layer F.Cu) (net 12) (tstamp 5F67D3A9))
  (via (at 152.4 91.44) (size 0.8) (drill 0.4) (layers F.Cu B.Cu) (net 12))
  (segment (start 147.32 91.44) (end 152.4 91.44) (width 0.25) (layer B.Cu) (net 12))
  (segment (start 193.2 99.06) (end 194.414001 100.274001) (width 0.25) (layer F.Cu) (net 13))
  (segment (start 194.414001 103.078357) (end 186.69 110.802358) (width 0.25) (layer F.Cu) (net 13))
  (segment (start 194.414001 100.274001) (end 194.414001 103.078357) (width 0.25) (layer F.Cu) (net 13))
  (segment (start 186.69 110.802358) (end 186.69 119.38) (width 0.25) (layer F.Cu) (net 13))
  (segment (start 186.69 119.38) (end 184.392999 121.677001) (width 0.25) (layer F.Cu) (net 13))
  (segment (start 184.392999 121.677001) (end 181.61 124.46) (width 0.25) (layer F.Cu) (net 13))
  (segment (start 181.61 124.46) (end 180.34 125.73) (width 0.25) (layer F.Cu) (net 13))
  (segment (start 180.34 125.73) (end 132.08 125.73) (width 0.25) (layer F.Cu) (net 13))
  (segment (start 132.08 125.73) (end 125.73 119.38) (width 0.25) (layer F.Cu) (net 13))
  (segment (start 125.73 119.38) (end 123.19 116.84) (width 0.25) (layer F.Cu) (net 13))
  (segment (start 123.19 116.84) (end 123.19 115.57) (width 0.25) (layer F.Cu) (net 13))
  (via (at 123.19 104.14) (size 0.8) (drill 0.4) (layers F.Cu B.Cu) (net 13))
  (segment (start 123.19 115.57) (end 123.19 115.57) (width 0.25) (layer F.Cu) (net 13) (tstamp 5F67B295))
  (via (at 123.19 115.57) (size 0.8) (drill 0.4) (layers F.Cu B.Cu) (net 13))
  (segment (start 123.19 104.14) (end 123.19 115.57) (width 0.25) (layer B.Cu) (net 13))
  (segment (start 123.19 104.14) (end 125.73 101.6) (width 0.25) (layer F.Cu) (net 13))
  (segment (start 120.65 102.87) (end 120.65 110.49) (width 0.25) (layer F.Cu) (net 15))
  (via (at 120.65 110.49) (size 0.8) (drill 0.4) (layers F.Cu B.Cu) (net 15))
  (segment (start 120.65 115.57) (end 120.65 115.57) (width 0.25) (layer F.Cu) (net 15) (tstamp 5F67B29D))
  (segment (start 120.65 110.49) (end 120.65 115.57) (width 0.25) (layer B.Cu) (net 15))
  (segment (start 120.65 115.57) (end 120.65 115.57) (width 0.25) (layer B.Cu) (net 15) (tstamp 5F67BD92))
  (via (at 120.65 115.57) (size 0.8) (drill 0.4) (layers F.Cu B.Cu) (net 15))
  (segment (start 120.65 102.87) (end 124.46 99.06) (width 0.25) (layer F.Cu) (net 15))
  (segment (start 124.46 99.06) (end 125.73 99.06) (width 0.25) (layer F.Cu) (net 15))
  (segment (start 96.52 99.06) (end 97.95 99.06) (width 0.25) (layer F.Cu) (net 15))
  (segment (start 120.65 116.586) (end 119.888 117.348) (width 0.25) (layer F.Cu) (net 15))
  (segment (start 120.65 115.57) (end 120.65 116.586) (width 0.25) (layer F.Cu) (net 15))
  (segment (start 119.888 117.348) (end 105.918 117.348) (width 0.25) (layer F.Cu) (net 15))
  (segment (start 105.918 117.348) (end 95.25 106.68) (width 0.25) (layer F.Cu) (net 15))
  (segment (start 95.25 100.33) (end 96.52 99.06) (width 0.25) (layer F.Cu) (net 15))
  (segment (start 95.25 106.68) (end 95.25 100.33) (width 0.25) (layer F.Cu) (net 15))
  (segment (start 107.95 99.06) (end 106.68 100.33) (width 0.25) (layer F.Cu) (net 17))
  (segment (start 106.68 100.33) (end 106.68 107.79) (width 0.25) (layer F.Cu) (net 17))
  (segment (start 125.73 96.52) (end 110.49 96.52) (width 0.25) (layer F.Cu) (net 17))
  (segment (start 110.49 96.52) (end 107.95 99.06) (width 0.25) (layer F.Cu) (net 17))
  (segment (start 195.605 98.917) (end 195.605 104.06) (width 0.25) (layer F.Cu) (net 29))
  (segment (start 193.198 96.51) (end 195.605 98.917) (width 0.25) (layer F.Cu) (net 29))
  (segment (start 199.335 107.79) (end 199.38 107.79) (width 0.25) (layer F.Cu) (net 29))
  (segment (start 195.605 104.06) (end 199.335 107.79) (width 0.25) (layer F.Cu) (net 29))
  (segment (start 102.87 83.82) (end 97.79 88.9) (width 0.25) (layer F.Cu) (net 29))
  (segment (start 97.948 89.058) (end 97.948 96.51) (width 0.25) (layer F.Cu) (net 29))
  (segment (start 97.79 88.9) (end 97.948 89.058) (width 0.25) (layer F.Cu) (net 29))
  (segment (start 100.4 104.06) (end 100.355 104.06) (width 0.25) (layer F.Cu) (net 29))
  (segment (start 104.13 107.79) (end 100.4 104.06) (width 0.25) (layer F.Cu) (net 29))
  (segment (start 100.355 98.917) (end 100.355 104.06) (width 0.25) (layer F.Cu) (net 29))
  (segment (start 97.948 96.51) (end 100.355 98.917) (width 0.25) (layer F.Cu) (net 29))
  (segment (start 165.11 96.51) (end 193.198 96.51) (width 0.25) (layer F.Cu) (net 29))
  (segment (start 157.48 104.14) (end 165.11 96.51) (width 0.25) (layer F.Cu) (net 29))
  (segment (start 151.13 104.14) (end 157.48 104.14) (width 0.25) (layer F.Cu) (net 29))
  (segment (start 123.19 83.82) (end 125.73 81.28) (width 0.25) (layer F.Cu) (net 29))
  (segment (start 102.87 83.82) (end 123.19 83.82) (width 0.25) (layer F.Cu) (net 29))
  (segment (start 151.13 104.14) (end 149.86 102.87) (width 0.25) (layer F.Cu) (net 29))
  (segment (start 149.86 100.33) (end 148.59 99.06) (width 0.25) (layer F.Cu) (net 29))
  (segment (start 149.86 102.87) (end 149.86 100.33) (width 0.25) (layer F.Cu) (net 29))
  (segment (start 148.59 99.06) (end 148.59 82.55) (width 0.25) (layer F.Cu) (net 29))
  (segment (start 127 82.55) (end 125.73 81.28) (width 0.25) (layer F.Cu) (net 29))
  (segment (start 148.59 82.55) (end 127 82.55) (width 0.25) (layer F.Cu) (net 29))
  (segment (start 170.24 113.224) (end 170.24 98.9) (width 0.25) (layer B.Cu) (net 31))
  (segment (start 117.674 114.3) (end 117.674 116.15) (width 0.25) (layer B.Cu) (net 31))
  (segment (start 164.592 118.872) (end 170.24 113.224) (width 0.25) (layer B.Cu) (net 31))
  (segment (start 120.396 118.872) (end 164.592 118.872) (width 0.25) (layer B.Cu) (net 31))
  (segment (start 117.674 116.15) (end 120.396 118.872) (width 0.25) (layer B.Cu) (net 31))
  (segment (start 180.99 112.46) (end 181.62 113.09) (width 0.25) (layer F.Cu) (net 32))
  (segment (start 180.99 98.9) (end 180.99 112.46) (width 0.25) (layer F.Cu) (net 32))
  (segment (start 167.43 98.9) (end 166.99 98.9) (width 0.25) (layer F.Cu) (net 36))
  (segment (start 166.99 105.96) (end 181.62 120.59) (width 0.25) (layer F.Cu) (net 36))
  (segment (start 166.99 98.9) (end 166.99 105.96) (width 0.25) (layer F.Cu) (net 36))
  (segment (start 177.74 98.9) (end 177.74 104.842) (width 0.25) (layer B.Cu) (net 37))
  (segment (start 198.628 125.73) (end 200.406 125.73) (width 0.25) (layer B.Cu) (net 37))
  (segment (start 177.74 104.842) (end 198.628 125.73) (width 0.25) (layer B.Cu) (net 37))
  (segment (start 191.444 113.03) (end 190.174 114.3) (width 0.25) (layer B.Cu) (net 38))
  (segment (start 200.406 113.03) (end 191.444 113.03) (width 0.25) (layer B.Cu) (net 38))

)
